%APPFAMILY%
0.4.1.9
Configuration and Monitoring
TCP/IP Connections
Data Connections
SystemMonitor
ObjectManager
Messages
Logging
Encrypt all connections to server
We recommend to check this for higher security by encrypted data transfers between client and server
Allow remote configuration through server
Only check this box if you trust the owner of the configured server, because then new IP connections can be established from this server to this client's LAN at any time
Auto Reconnect
If checked this TCP client will retry to connect every minute to the server and reactivate all locally configured forward jobs on the server
Configuration
Control connection to IPrAcc TCP Server
Server password:
Enter the password here that is required for dialing into the server. If necessary, ask the operator of the server for this password.
Enter here the IP address or DNS name of the IPrAcc TCP server you want to connect with
Enter here the TCP/IP port for the control connection to the IPrAcc TCP server you want to connect with
Forward Jobs  --->   forward TCP connections incoming on    IPrAcc TCP Server : Server Port    to    Destination IP Address : Destination Port
Enter all desired forwardings in the following table. Button ---> activates the forwarding, -||- stops the forwarding.
Show server info
for
Allow only encrypted connections from clients
Automatically disconnect after
seconds of idle time
WhiteList - List of allowed IP addresses
If you enter at least one IP address in the following list, connections from the IPrAcc server to this client are only permitted from the IP addresses listed here
Cancel
Apply
Configuration file
Unique ID
RCP Password
Enter a strong password here. Clients can only establish connections to this server with this password.
Listen for Clients
The configuration data of this application is stored in this file
Disconnect all Clients
Attention: Do you really want to interrupt all ongoing connections?
Designation
This application is displayed with this designation in the tables of the connection partners
Send DNS information to remote sites
With this checkbox you determine whether this application is allowed to send DNS information about the devices involved in the configured forwarding from this network to the remote stations. This is an advantage for a better overview and faster error analysis, but internal information from this network may be passed on to the remote stations. Therefore, before setting this checkbox, obtain the consent of the owner of this network!
Update tables cyclically
Check this box if you want to save on the computing power that is required for regularly updating the tables
Make all columns in this table visible
Collapse the not so important columns in this table for a better overview
Send error message after
seconds connection interruption
Routine messages Interval [min]
Target directory for message files
This table shows detailed information about all connections to IPrAcc clients
This table shows detailed information about all forwarding jobs
This table shows detailed information about all current data connections
Define, control and monitor all the forwarding jobs you need with this table
Show all data con- nections
Reserved Ports
Here you can specify which ports should be blocked so that clients cannot use them.
First enter the port or port range you wish to add in the text field to the right of this button
First enter the port or range of ports you wish to delete in the text box to the left of this button.
Display actual messages of this software
Displays a table with all IP sockets and status of all connections
Displays a table with all software objects currently used in this application to monitor them
With this window you can monitor important system ressources for always reliable operation if this software
Display actual log outputs of this software
Merge port ranges to: %0
Remove individual port %0
Suggestions for improvements:
Apply changes?
Do you really want to delete all entries?
Add a port or port range
Delete selected entry
Delete all entries
If this checkbox is set, the list works as a “whitelist”, i.e. only the ports selected here are enabled for the clients
IP address from network adaptor, from which data should be received. Use 0.0.0.0 to receive data from any available network adaptor.
Optimisation suggestions for the port list